{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["系统架构图（正式环境）","服务器配置（正式环境）","服务器配置（测试环境）","服务器配置（开发环境）"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"系统架构图（正式环境）","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"服务器配置（正式环境）","index":1,"n_rows":16,"n_cols":10,"rows_kept":16,"cut":false,"hidden":false,"merged":[[0,3,0,8],[11,1,15,1],[3,2,4,2],[5,2,6,2],[7,2,8,2],[9,2,10,2],[3,1,10,1],[13,2,14,2],[13,8,14,8]]}
[null,null,null,"服务器配置信息"]
[null,"类别","用途","数量",null,"操作系统","硬盘","内部端口","说明","基本配置"]
[null,"负载类服务器","负载",{"$nulls":5},"负载均衡（使用客户现有环境）"]
[null,"应用类服务器","C1 Web",1,"S-C1-Web-A01","Windows Server 2012 R2 Standard",">300（C=100GB, D=200GB）",9510,"2台部署负载均衡","Intel®Xeon® cpu E5 2690 v4（16核）       32G"]
[null,null,null,1,"S-C1-Web-A02","Windows Server 2012 R2 Standard",">300（C=100GB, D=200GB）",9510,"2台部署负载均衡","Intel®Xeon® cpu E5 2690 v4（16核）       32G"]
[null,null,"主数据Web",1,"S-C1-Web-B01","Linux",">300（系统盘=100GB, 数据盘=200GB）",80,"2台部署负载均衡","Intel®Xeon® cpu E5 2690 v4（8核）        16G"]
[null,null,null,1,"S-C1-Web-B02","Linux",">300（系统盘=100GB, 数据盘=200GB）",80,"2台部署负载均衡","Intel®Xeon® cpu E5 2690 v4（8核）        16G"]
[null,null,"主数据API",1,"S-C1-API-01","Linux",">300（系统盘=100GB, 数据盘=200GB）",80,"2台部署负载均衡","Intel®Xeon® cpu E5 2690 v4（16核）       32G"]
[null,null,null,1,"S-C1-API-02","Linux",">300（系统盘=100GB, 数据盘=200GB）",80,"2台部署负载均衡","Intel®Xeon® cpu E5 2690 v4（16核）       32G"]
[null,null,"C1 BA",1,"S-C1-BA-01","Linux Cent OS 7",">1000（根分区100G,逻辑分区900GB）",80,"2台部署负载均衡","Intel®Xeon® cpu E5 2690 v4（16核）       64G"]
[null,null,null,1,"S-C1-BA-02","Linux Cent OS 7",">1000（根分区100G,逻辑分区900GB）",80,"2台部署负载均衡","Intel®Xeon® cpu E5 2690 v4（16核）       64G"]
[null,"数据存贮类服务器","C1 TABase Server",1,"S-C1-TABase-01","Windows Server 2012 Standard",">300（C=100GB, D=200GB）",5495,null,"Intel®Xeon® cpu E5 2690 v4（32核）       256G"]
[null,null,"缓存服务器",1,"S-C1-Cache-01","Windows Server 2012 R2 Standard",">300（C=100GB, D=200GB）",null,null,"Intel®Xeon® cpu E5 2690 v4（16核）       32G"]
[null,null,"DB Server",1,"S-C1-DB-01","Windows Server 2012 Standard",">300（C=100GB, D=200GB）",1433,"SQL SERVER2008R2及以上，2台部署Alwayson","Intel®Xeon® cpu E5 2690 v4（16核）       32G"]
[null,null,null,1,"S-C1-DB-02","Windows Server 2012 Standard",">300（C=100GB, D=200GB）",1433,null,"Intel®Xeon® cpu E5 2690 v4（16核）       32G"]
[null,null,"文件服务器",{"$nulls":5},"NAS（使用客户现有环境）"]

{"sheet":"服务器配置（测试环境）","index":2,"n_rows":11,"n_cols":13,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,3,0,9],[6,1,8,1],[2,1,5,1],[6,6,7,6],[3,6,5,6]]}
[null,null,null,"服务器配置信息"]
[null,"类别","用途","数量","主机名","IP地址","账号密码","操作系统","硬盘","内部端口","说明","基本配置"]
[null,"应用类服务器","C1 Web",1,"TEST-C1-Web-A01","192.168.209.171","用户名：testc1 \n密码：123qwe!@#","Windows Server 2012 R2 Standard",">200（C=100GB, D=100GB）",9510,null,"Intel®Xeon® cpu E5 2690 v4（8核）       16G"]
[null,null,"主数据Web",1,"TEST-C1-Web-B01","192.168.209.172","SSH端口：8022\n用户名：root\n密码：aoyuan.3883","Linux",">200（系统盘=100GB, 数据盘=100GB）",80,null,"Intel®Xeon® cpu E5 2690 v4（8核）       16G"]
[null,null,"主数据API兼缓存服务器",1,"TEST-C1-API-01","192.168.209.173",null,"Linux",">200（系统盘=100GB, 数据盘=100GB）",80,null,"Intel®Xeon® cpu E5 2690 v4（8核）       16G"]
[null,null,"C1 BA",1,"TEST-C1-BA-01","192.168.209.174",null,"Linux Cent OS 7",">400（根分区100G,逻辑分区300GB）",80,null,"Intel®Xeon® cpu E5 2690 v4（8核）       32G"]
[null,"数据存贮类服务器","C1 TABase Server",1,"TEST-C1-TA-01","192.168.209.175","用户名：testc1 \n密码：123qwe!@#","Windows Server 2012 Standard",">300（C=100GB, D=200GB）",5495,null,"Intel®Xeon® cpu E5 2690 v4（8核）       64G"]
[null,null,"DB Server",1,"TEST-C1-DB-01","192.168.209.176",null,"Windows Server 2012 Standard",">300（C=100GB, D=200GB）",1433,"SQL SERVER2008R2及以上","Intel®Xeon® cpu E5 2690 v4（8核）       16G","db_master_data\n123456"]
[null,null,"NAS文件服务器",{"$nulls":7},"NAS（使用客户现有环境）"]
[]
[null,null,"http://192.168.209.174/editor/10886/explore/1\n账号：ba\n密码：ba"]

{"sheet":"服务器配置（开发环境）","index":3,"n_rows":8,"n_cols":9,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,3,0,6],[2,1,4,1],[5,1,7,1]]}
[null,null,null,"服务器配置信息"]
[null,"类别","用途","数量","操作系统","硬盘","内部端口","说明","基本配置"]
[null,"应用类服务器","C1 Web",1,"Windows Server 2012 R2 Standard",">200（C=100GB, D=100GB）",9510,null,"Intel®Xeon® cpu E5 2690 v4（8核）       16G"]
[null,null,"主数据Web与API与缓存服务器",1,"Linux",">200（系统盘=100GB, 数据盘=100GB）",80,null,"Intel®Xeon® cpu E5 2690 v4（8核）       32G"]
[null,null,"C1 BA",1,"Linux Cent OS 7",">400（根分区100G,逻辑分区300GB）",80,null,"Intel®Xeon® cpu E5 2690 v4（8核）       32G"]
[null,"数据存贮类服务器","C1 TABase Server",1,"Windows Server 2012 Standard",">300（C=100GB, D=200GB）",5495,null,"Intel®Xeon® cpu E5 2690 v4（8核）       64G"]
[null,null,"DB Server",1,"Windows Server 2012 Standard",">300（C=100GB, D=200GB）",1433,"SQL SERVER2008R2及以上","Intel®Xeon® cpu E5 2690 v4（8核）       16G"]
[null,null,"NAS文件服务器",{"$nulls":4},"NAS（使用客户现有环境）"]